AVR Libc Home Page |  | AVR Libc Development Pages
Main Page | User Manual | Library Reference | FAQ | Alphabetical Index | Example Projects

# <avr/sleep.h>: Power Management and Sleep Modes

## Detailed Description

     #include <avr/sleep.h>

Use of the `SLEEP` instruction can allow an application to reduce its power comsumption considerably. AVR devices can be put into different sleep modes. Refer to the datasheet for the details relating to the device you are using.

There are several macros provided in this header file to actually put the device into sleep mode. The simplest way is to optionally set the desired sleep mode using `set_sleep_mode()` (it usually defaults to idle mode where the CPU is put on sleep but all peripheral clocks are still running), and then call `sleep_mode()`. This macro automatically sets the sleep enable bit, goes to sleep, and clears the sleep enable bit.

Example:

        #include <avr/sleep.h>

        ...
          set_sleep_mode(<mode>);
          sleep_mode();

Note that unless your purpose is to completely lock the CPU (until a hardware reset), interrupts need to be enabled before going to sleep.

As the `sleep_mode()` macro might cause race conditions in some situations, the individual steps of manipulating the sleep enable (SE) bit, and actually issuing the `SLEEP` instruction, are provided in the macros `sleep_enable()`, `sleep_disable()`, and `sleep_cpu()`. This also allows for test-and-sleep scenarios that take care of not missing the interrupt that will awake the device from sleep.

Example:

        #include <avr/interrupt.h>
        #include <avr/sleep.h>

        ...
          set_sleep_mode(<mode>);
          cli();
          if (some_condition)
          {
            sleep_enable();
            sei();
            sleep_cpu();
            sleep_disable();
          }
          sei();

This sequence ensures an atomic test of `some_condition` with interrupts being disabled. If the condition is met, sleep mode will be prepared, and the `SLEEP` instruction will be scheduled immediately after an `SEI` instruction. As the intruction right after the `SEI` is guaranteed to be executed before an interrupt could trigger, it is sure the device will really be put to sleep.

## Functions
void | sleep_enable (void)
void | sleep_disable (void)
void | sleep_cpu (void)

## Function Documentation

void sleep_cpu | ( | void |  | ) |

Put the device into sleep mode. The SE bit must be set beforehand, and it is recommended to clear it afterwards.

void sleep_disable | ( | void |  | ) |

Clear the SE (sleep enable) bit.

void sleep_enable | ( | void |  | ) |

Put the device in sleep mode. How the device is brought out of sleep mode depends on the specific mode selected with the set_sleep_mode() function. See the data sheet for your device for more details.

Set the SE (sleep enable) bit.

Automatically generated by Doxygen 1.5.6 on 4 Dec 2008.