Arduino

Reference Language | Libraries | Comparison | Changes

## Arduino/Processing Language Comparison

The Arduino language (based on Wiring) is implemented in C/C++, and therefore has some differences from the Processing language, which is based on Java.

### Arrays

Arduino | Processing
int bar[8]; bar[0] = 1; | int[] bar = new int[8]; bar[0] = 1;
int foo[] = { 0, 1, 2 }; | int foo[] = { 0, 1, 2 }; or int[] foo = { 0, 1, 2 };

### Loops

Arduino | Processing
int i; for (i = 0; i < 5; i++) { ... } | for (int i = 0; i < 5; i++) { ... }

### Printing

Arduino | Processing
Serial.println("hello world"); | println("hello world");
int i = 5; Serial.println(i); | int i = 5; println(i);
int i = 5; Serial.print("i = "); Serial.print(i); Serial.println(); | int i = 5; println("i = " + i);

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes