Building the bootloader for the LilyPadUSB
1. Download the LUFA-111009 file (http://fourwalledcubicle.com/blog/2011/10/lufa-111009-released/).
2. Extract that file directly to the Caterina-LilyPadUSB bootloader directory.
3. Open a command prompt in the Caterina-LilyPadUSB bootloader directory.
4. Type 'make'.
5. Enjoy!

Programming the bootloader for the LilyPadUSB
1. Open a command prompt in the Caterina-LilyPadUSB folder.
2. Connect your programmer- use a 2x3 .1" header, pressed against the programming vias.
3. Type 'make program' into the command prompt.