Arduino

Reference Language | Libraries | Comparison | Changes

## if (conditional) and ==, !=, <, > (comparison operators)

`if`, which is used in conjunction with a comparison operator, tests whether a certain condition has been reached, such as an input being above a certain number. The format for an if test is:

    if (someVariable > 50)
    {
      // do something here
    }

The program tests to see if someVariable is greater than 50. If it is, the program takes a particular action. Put another way, if the statement in parentheses is true, the statements inside the brackets are run. If not, the program skips over the code.

The brackets may be omitted after an if statement. If this is done, the next line (defined by the semicolon) becomes the only conditional statement.

    if (x > 120) digitalWrite(LEDpin, HIGH);

    if (x > 120)
    digitalWrite(LEDpin, HIGH);

    if (x > 120){ digitalWrite(LEDpin, HIGH); }

    if (x > 120){
      digitalWrite(LEDpin1, HIGH);
      digitalWrite(LEDpin2, HIGH);
    }                                 // all are correct

The statements being evaluated inside the parentheses require the use of one or more operators:

### Comparison Operators:

     x == y (x is equal to y)
     x != y (x is not equal to y)
     x <  y (x is less than y)
     x >  y (x is greater than y)
     x <= y (x is less than or equal to y)
     x >= y (x is greater than or equal to y)

#### Warning:

Beware of accidentally using the single equal sign (e.g.`if (x = 10)` ). The single equal sign is the assignment operator, and sets x to 10 (puts the value 10 into the variable x). Instead use the double equal sign (e.g.`if (x == 10)` ), which is the comparison operator, and tests whether x is equal to 10 or not. The latter statement is only true if x equals 10, but the former statement will always be true.

This is because C evaluates the statement `if (x=10)` as follows: 10 is assigned to x (remember that the single equal sign is the assignment operator), so x now contains 10. Then the 'if' conditional evaluates 10, which always evaluates to TRUE, since any non-zero number evaluates to TRUE. Consequently, `if (x = 10)` will always evaluate to TRUE, which is not the desired result when using an 'if' statement. Additionally, the variable x will be set to 10, which is also not a desired action.

if can also be part of a branching control structure using the if...else] construction.

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes