Next: Assembler, Previous: Side Effects, Up: RTL

### 12.16 Embedded Side-Effects on Addresses

Six special side-effect expression codes appear as memory addresses.

`(pre_dec:`m x`)`
  Represents the side effect of decrementing x by a standard amount and represents also the value that x has after being decremented. x must be a `reg` or `mem`, but most machines allow only a `reg`. m must be the machine mode for pointers on the machine in use. The amount x is decremented by is the length in bytes of the machine mode of the containing memory reference of which this expression serves as the address. Here is an example of its use:

                (mem:DF (pre_dec:SI (reg:SI 39)))

  This says to decrement pseudo register 39 by the length of a `DFmode` value and use the result to address a `DFmode` value.

`(pre_inc:`m x`)`
  Similar, but specifies incrementing x instead of decrementing it.

`(post_dec:`m x`)`
  Represents the same side effect as `pre_dec` but a different value. The value represented here is the value x has before being decremented.

`(post_inc:`m x`)`
  Similar, but specifies incrementing x instead of decrementing it.

`(post_modify:`m x y`)`
  Represents the side effect of setting x to y and represents x before x is modified. x must be a `reg` or `mem`, but most machines allow only a `reg`. m must be the machine mode for pointers on the machine in use.

  The expression y must be one of three forms:

  `(plus:`m x z`)`, `(minus:`m x z`)`, or `(plus:`m x i`)`,
  where z is an index register and i is a constant.

  Here is an example of its use:

                (mem:SF (post_modify:SI (reg:SI 42) (plus (reg:SI 42)
                                                          (reg:SI 48))))

  This says to modify pseudo register 42 by adding the contents of pseudo register 48 to it, after the use of what ever 42 points to.

`(pre_modify:`m x expr`)`
  Similar except side effects happen before the use.

These embedded side effect expressions must be used with care. Instruction patterns may not use them. Until the flow pass of the compiler, they may occur only to represent pushes onto the stack. The flow pass finds cases where registers are incremented or decremented in one instruction and used as an address shortly before or after; these cases are then transformed to use pre- or post-increment or -decrement.

If a register used as the operand of these expressions is used in another address in an insn, the original value of the register is used. Uses of the register outside of an address are not permitted within the same insn as a use in an embedded side effect expression because such insns behave differently on different machines and hence must be treated as ambiguous and disallowed.

An instruction that can be represented with an embedded side effect could also be represented using `parallel` containing an additional `set` to describe how the address register is altered. This is not done because machines that allow these operations at all typically allow them wherever a memory address is called for. Describing them as additional parallel stores would require doubling the number of entries in the machine description.