Arduino

Reference Language | Libraries | Comparison | Changes

## word

#### Description

A word stores a 16-bit unsigned number, from 0 to 65535. Same as an unsigned int.

#### Example

        word w = 10000;

#### See also

- byte
- word()

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes