Arduino

Reference Language | Libraries | Comparison | Changes

## sizeof

#### Description

The sizeof operator returns the number of bytes in a variable type, or the number of bytes occupied by an array.

#### Syntax

sizeof(variable)

#### Parameters

variable: any variable type or array (e.g. int, float, byte)

#### Example code

The sizeof operator is useful for dealing with arrays (such as strings) where it is convenient to be able to change the size of the array without breaking other parts of the program.

This program prints out a text string one character at a time. Try changing the text phrase.

    char myStr[] = "this is a test";
    int i;

    void setup(){
      Serial.begin(9600);
    }

    void loop() {
      for (i = 0; i < sizeof(myStr) - 1; i++){
        Serial.print(i, DEC);
        Serial.print(" = ");
        Serial.write(myStr[i]);
        Serial.println();
      }
      delay(5000); // slow down the program
    }

Note that sizeof returns the total number of bytes. So for larger variable types such as ints, the for loop would look something like this. Note also that a properly formatted string ends with the NULL symbol, which has ASCII value 0.

    for (i = 0; i < (sizeof(myInts)/sizeof(int)) - 1; i++) {
      // do something with myInts[i]
    }

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes