Next: WIN32, Previous: SPU ELF, Up: Machine Dependent

### 4.12 ld's Support for Various TI COFF Versions

The --format switch allows selection of one of the various TI COFF versions. The latest of this writing is 2; versions 0 and 1 are also supported. The TI COFF versions also vary in header byte-order format; ld will read any version or byte order, but the output header format depends on the default specified by the specific target.